
--------------------------------------------------------------------------------
SNC-RZ30/2 series firmware release notes 
--------------------------------------------------------------------------------

Ver3.14(Aug 9, 2007)
* Bug fix for wireless function which doesn't set WEP key correctly in some cases.
* Bug fix for malfunction of web access from a client PC in which .NET framework
  3.0 is installed.
* Windows Vista support


Ver3.10(Oct 12, 2006)
* Setting a NTP synchronization and FTP client schedules for a 
  periodical image sending, during the schedules, turned off 
  the power and turned on, the periodical image sending was not 
  recovered. This malfunction was fixed.
* By the Windows Update program, Internet Explorer requested to 
  activate the window showing white border lines. Activation is 
  not needed with this version.

CAUTION : 
  Applying this version, you CAN NOT go back to less than V3.10.


Ver3.03
* Bug fix for hang-up problem when the camera received frequent sensor inputs.
* Addition of Pan and Tilt motor initialization when the camera is rebooted.
* Fixed a bug which is related to Day/Night auto mode.
* Bug fix for hang-up when some PTZ operation is made during tour operation.
* Bug fix for Trigger/Area setting/Activity detection not working via a proxy
  server with SunJava 1.4.2 or later.
* Bug fix for the command "/command/main.cgi?trigger=alarmout2on/off"
* Modification of some discordance when Mount=desktop is set.

Ver3.02
* Bug fix for the time-out problem when Pan operation is made with minimum speed
* GUI modification in accordance with IPELA branding (RealShot logos are deleted.)

Ver3.01
* First release for SNC-RZ30/2
* E-flip function is newly supported.
* CamPos header functionality is newly supported.
* The following FTP client functionality is newly supported.
  - "FcStoreMode=rename1" parameter which will make it not to delete
    the assigned file name.
* The following FTP server functionality is newly supported.
  - Change of FTP port numbers
  - Passive mode support
* Bug fix for FTP client function when the camera fail to acquire the cilent port number
  which is already used by another application
* Some modification in terms of DHCP implementation
